AT

* Meaning: "Attention" command – a basic check to see if the module is responsive.
* Response: OK – indicates the module is working and ready to receive commands.

ATI

* Meaning: "Attention – Identify" – requests device information such as model number or firmware version.
* Response: C102 – this is likely the model number or firmware ID of the module.

ATZ

* Meaning: "Reset" – resets the modem to its default configuration (soft reset).
* Response: OK – the command was accepted and the reset was successful.

